Check DDS signal fed into PA around 200 mVpp
yes
Check TTL lines are good.
yes
Check 50 dB attenuated output of PA
Voltage cut in half.
Rturn loss measurement of antenna 5
It's good (bryan checked)
Check 0-amplitude-fed PA output, look for transition of dupe.
Good
Turn on PA for 5000, 10000, 15k
5000 -> 150 mVpp
10000 -> 500 mVpp
15000 -> 900 mVpp
0003 screenshot of max power (15000)
0002 and 0001 are no power, toggle only